{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":20,"rows_kept":13,"merged":[[0,1,0,16],[2,0,2,5],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,3,19],[4,4,4,5],[4,6,4,7],[4,8,4,9],[4,10,4,11],[4,12,4,13],[4,14,4,15],[4,16,4,17],[4,18,4,19],[6,5,10,5],[6,7,10,7],[6,9,10,9],[6,11,10,11],[6,13,10,13],[6,15,10,15],[6,17,10,17],[6,19,10,19],[11,10,11,16],[12,0,12,19]],"flags":["formulas_cached_only"]}
[null,"盐边县2020年（三季度）城区生活饮用水水质监测结果"]
[]
["检验单位：盐边县疾病预防控制中心"]
["序号","监测点","生产单位","水样类型","检    测    项    目    及    结    果"]
[{"$nulls":4},"菌落总数（CFU/ml）",null,"总大肠菌群（MPU/100ml）",null,"色度（度）",null,"浑浊度（NTU）",null,"嗅和味（描述）",null,"肉眼可见物（描述）",null,"耗氧量（mg/L）",null,"氨氮（mg/L）"]
[{"$nulls":4},"检测结果","标准限值","检测结果","标准限值","检测结果","标准限值","检测结果","标准限值","检测结果","标准限值","检测结果","标准限值","检测结果","标准限值","检测结果","标准限值"]
[1,"盐边县幼儿园","盐边县自来水厂","末梢水",5,500,"未检出","不得检出","＜5",15,0.38,1,"无 ","无异臭异味","无","无",1.13,3,"＜0.02",0.5]
[2,"新城一小","盐边县自来水厂","末梢水",6,null,"未检出",null,"＜5",null,0.64,null,"无 ",null,"无",null,0.67,null,"＜0.02"]
[3,"民族中学","盐边县自来水厂","末梢水",2,null,"未检出",null,"＜5",null,0.33,null,"无 ",null,"无",null,0.87,null,"＜0.02"]
[4,"盐边县中学","盐边县自来水厂","末梢水",17,null,"未检出",null,"＜5",null,0.44,null,"无 ",null,"无",null,0.64,null,"＜0.02"]
[5,"金谷苑小区","盐边县自来水厂","二次供水",39,null,"未检出",null,"＜5",null,0.72,null,"无",null,"无",null,0.65,null,"＜0.02"]
["采样人员：陈江龙  杜思璇",{"$nulls":9},"采样时间：2020 年 7 月 20 日"]
["注：（1）水质指标的检验和结果评价按照《生活饮用水卫生标准》（GB5749-2006）、《生活饮用水标准检验方法》（GB/T5750-2006）执行。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}