{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":58,"n_cols":9,"rows_kept":58,"merged":[[0,0,0,8],[57,0,57,4]],"flags":["formulas_cached_only"]}
["2024年攀枝花市盐边生态环境监测站仪器设备检定清单"]
["序号","仪器名称","型号规格","出厂编号","制造厂","数量","服务方式","检定参数","备注"]
[1,"智能TSP综合采样器","崂应2050型","Q31031262","青岛崂应应用技术研究所","1台","现场/送检","流量、大气压"]
[2,"智能TSP综合采样器","崂应2050型","Q31025621","青岛崂应应用技术研究所","1台",null,"流量、大气压"]
[3,"风速仪","DHC100",20210804684,null,"1台",null,"风速、气温"]
[5,"自动烟尘烟气综合测试仪","ZR-3260","3260A17102889","青岛众瑞智能仪器有限公司","1台",null,"流量、大气压、二氧化硫、一氧化氮、二氧化氮、一氧化碳、氧含量"]
[6,"自动烟尘烟气综合测试仪","ZR-3260","3260A17102902","青岛众瑞智能仪器有限公司","1台",null,"流量、大气压、二氧化硫、一氧化氮、二氧化氮、一氧化碳、氧含量"]
[7,"高原空盒气压表","DMY3-1",100994,"长春气象仪器有限公司","1台",null,"大气压"]
[8,"高原空盒气压表","DMY3-2",101075,"长春气象仪器有限公司","1台",null,"大气压"]
[9,"便携式余氯测试仪","DR300","20100A000118","HACH","1台",null,"总氯、游离氯"]
[10,"声级计","AWA6228+","00310403","杭州爱华仪器有限公司","1台",null,"噪声","检定"]
[11,"声校准器","AWA6021A",1007515,"杭州爱华仪器有限公司","1台",null,"声校准值","检定"]
[12,"烟尘（气）测试校准仪","崂应7050",15060492,"青岛崂应应用技术研究所","1台"]
[13,"孔口流量校准器","崂应7020Z",11110183,"青岛崂应应用技术研究所","1台",null,"流量"]
[14,"智能皂膜流量计","崂应7030",11090230,"青岛崂应应用技术研究所","1台",null,"流量"]
[15,"雷磁便携式浊度计","DGB-175",6.70900500210901e+16,"上海仪电科仪","1台",null,"浊度"]
[16,"雷磁便携式浊度计","DGB-175",6.70900500210901e+16,"上海仪电科仪","1台",null,"浊度"]
[17,"便携式色度计","WZB-175","652000S0021090042","上海仪电科仪","1台",null,"色度"]
[18,"便携式色度计","WZB-175","652000S0021090030","上海仪电科仪","1台",null,"色度"]
[19,"便携式多参数分析仪","DZB-712F","651820N0021100031","上海仪电科仪","1台",null,"PH、溶解氧、电导、温度"]
[20,"便携式多参数分析仪","DZB-712F","651820N0021100023","上海仪电科仪","1台",null,"PH、溶解氧、电导、温度"]
[21,"连续流动分析仪","Futura","17-1243-1/3","AMS Alliance","1台",null,"挥发酚、氰化物"]
[22,"气相分子吸收光谱仪","GMA3386A","11200444A001","上海北裕分析仪器股份有限公司","1台"]
[23,"可见分光光度计","VIS-723N","100765","北京瑞利分析仪器公司","1台",null,"分光值"]
[24,"紫外可见分光光度计","UV Power","300472","北京莱伯泰科仪器有限公司","1台",null,"分光值"]
[25,"原子荧光光度计","AFS-930","930-15051161","北京吉天仪器有限公司","1台"]
[26,"生化培养箱","LBI-80-D2","07091706-1","上海龙跃","1台"]
[27,"生化培养箱","LBI-80-D2","07091706-2","上海龙跃","1台"]
[28,"生化培养箱","SPX-200F-Ⅱ",10041704,"上海龙跃仪器设备有限公司","1台"]
[29,"电热恒温水浴锅","DK-98-ⅡA",2004206,"天津市泰斯特仪器有限公司","1台"]
[30,"电热恒温水浴锅","DK-99-ⅡA",2101212,"天津市泰斯特仪器有限公司","1台"]
[31,"电子天平","ESJ200-4","070839","沈阳龙腾电子有限公司","1台",null,"重量","检定"]
[32,"电子天平","MS105DU","B708741037","梅特勒.托利多","1台",null,"重量","检定"]
[33,"电子天平","AXB6002,C3-6699-12",null,null,"1台",null,"重量","检定"]
[34,"恒温恒湿自动称重系统","RG-AWS8","RGAWS8000","青岛容广电子技术有限公司","1台"]
[35,"全自动紫外测油仪","博海UV3000B",2011854,null,"1台"]
[36,"电热恒温鼓风干燥箱","101-2-3-Ⅱ","000008225","上海跃进医疗器械厂","1台"]
[37,"电热鼓风干燥箱","泰斯特WGL-125B",2106017,"天津市泰斯特仪器有限公司","1台"]
[38,"流量计","ALICAT  62A/62AW系列","62AW-1-00-1-25-KM6011\n62A-1-00-0-200-KM6001","艾里卡特Alicat","1套",null,"流量"]
[39,"立式高压蒸汽灭菌器","申安LDZX-50L",null,null,"1台"]
[40,"雷磁多参数分析仪","DZB-708F","651219S0121080009","上海仪电科仪","1台",null,"PH、溶解氧、电导、温度"]
[41,"雷磁多参数分析仪","DZB-708F","65219S0121080005","上海仪电科仪","1台",null,"PH、溶解氧、电导、温度"]
[42,"机械温湿度表","WS-D2","01","上海天宇科技仪表有限公司","1台",null,"温度、湿度"]
[43,"机械温湿度表","WS-D2","02","上海天宇科技仪表有限公司","1台",null,"温度、湿度"]
[44,"数字温度计","TP102",null,null,"1台",null,"温度"]
[45,"数字温度计","TP103",null,null,"1台",null,"温度"]
[46,"玻璃液体温度计","棒式",null,null,"4台",null,"温度"]
[47,"小米温湿度表","YLWSDCGQ",null,null,"7台",null,"温度、湿度"]
[48,"低浓度自动烟尘烟气综合测试仪","ZR-3260D型","3260DA22122195","青岛众瑞智能仪器有限公司","1台",null,"二氧化硫、氮氧化物、一氧化碳、流量、大气压、氧含量"]
[49,"便携式紫外烟气综合分析仪","ZR-3211H型","3211H22094130","青岛众瑞智能仪器有限公司","1台",null,"二氧化硫、氮氧化物、一氧化碳、流量"]
[50,"阻容式烟气含湿量测试仪","ZR-D13E型","D13E22124414","青岛众瑞智能仪器有限公司","1台",null,"含湿量"]
[51,"环境空气颗粒物综合采样器","ZR-3929型","3923A22115978","青岛众瑞智能仪器有限公司","1台",null,"流量、大气压"]
[52,"环境空气颗粒物综合采样器","ZR-3929型","3923A22115960","青岛众瑞智能仪器有限公司","1台",null,"流量、大气压"]
[53,"紫外烟气分析仪","崂应3023Y型","2B04032490","青岛崂应环境科技有限公司","1台",null,"二氧化硫、氮氧化物、一氧化碳、流量"]
[54,"离子色谱仪","DIONEX AQUION",170921695,"Thermo",1]
[55,"表层水温表",{"$nulls":3},2]
[56,"总磷总氮多参数水质分析仪","AQ3700",null,"赛默飞世尔",1]
["合计",{"$nulls":4},"65台"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}